{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Tranchants"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tranchants","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[[20,1,20,2],[20,3,20,4],[4,3,4,5],[4,6,4,7],[11,1,11,2],[11,6,11,7],[7,6,7,8],[8,6,8,8],[9,6,9,8],[10,1,10,2],[6,6,6,9],[6,1,6,3],[7,1,7,2],[8,1,8,2],[9,1,9,2]]}
[]
[null,null,null,null,null,"Enveloppe de Calcul du Diagramme des Efforts Tranchants"]
[null,null,null,null,null,"Selon les RPA 2024"]
[null,null,null,null,null,"Valable uniquement pour les systèmes à contrevetent mixte"]
[null,null,null,"abdellatif-megnounif.com",null,null,"mescours∖RPA2024"]
[]
[null,"Données du mur voile",null,null,null,null,"Quelques vérifications "]
[null,"Largeur du mur (m) : lw=",null,3,null,null,"Voile ? 𝒍𝒘 ≥ 𝐦𝐚𝐱(𝐡𝐞/𝟑, 𝟒 𝐛𝐰 , 𝟏 𝐦) ?",null,null,"Verifiee"]
[null,"Epaisseur du mur (m) : bw=",null,0.2,null,null,"bw_min ? 𝒃𝒘 ≥ 𝒎𝒂𝒙(𝟏𝟓 𝒄𝒎,   𝒉𝒆/𝟐𝟎) ?",null,null,"Verifiee"]
[null,"Hauteur totale du mur (m) : hw=",null,9,null,null,"Elancement ? 𝒉𝒘/𝒍𝒘 > 𝟐.𝟎 ?",null,null,"Elance"]
[null,"Hauteur libre d'étage (m) : he=",null,3]
[null,"Nombre d'étages : Nb_etages =",null,3,null,null,"1/3 de Hw"]
[null,null,null,null,null,null,"hw3 =",3]
[]
[null,"Niveau","Hauteur (m)","Efforts tranchants (KN)","Efforts tranchants a 40%"]
[null,0,0,22,30.799999999999997]
[null,1,3,15,21]
[null,2,6,5,7]
[null,3,9,-2,-2.8]
[]
[null,"Droite a Hw/3",null,"Donnees des efforts finaux"]
[null,"Efforts tranchants (KN)","hauteur(m)","Nouvelle hauteur (m)","Efforts tranchants finaux (KN)"]
[null,30.799999999999997,3,0,30.799999999999997]
[null,21,3,3,21]
[null,7,3,3,21]
[null,-2.8,3,6,18.2]
[null,null,null,9,15.4]