{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Principal"],"not_rendered":{"charts":0,"images":17,"macros":1,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Principal","index":0,"n_rows":21,"n_cols":15,"rows_kept":21,"cut":false,"hidden":false,"merged":[[13,5,13,7],[19,11,19,12],[19,13,19,14],[19,3,19,8],[19,9,19,10],[1,2,3,7],[6,1,6,3],[10,1,10,2],[11,1,11,2],[12,1,12,2],[8,5,8,7],[12,5,12,7],[10,5,10,7],[11,5,11,7],[9,5,9,7],[16,1,16,2],[13,1,13,2],[17,1,17,2],[14,1,14,2],[15,1,15,2]]}
[]
[null,null,"Justifications de la sécurité selon les recommandations - RPA 2024"]
[]
[]
[null,null,null,"abdellatif-megnounif.com",null,"Mes cours\\RPA2024"]
[]
[null,"Données de la structure"]
[null,"hauteur totale (m) : hw="]
[null,"Nombre total d'étages",null,null,null,"Justification vis-à-vis de l'effet noyau",null,null,"(§ 5.5)"]
[null,"Valeur de l'amortissement (%)",null,null,null,"Justification vis-à-vis de l'équilibre d'ensemble (Renversement)",null,null,"(§ 5.5)"]
[null,"Coefficient de zone A",null,null,null,"Justification vis-à-vis de la résistance des planchers",null,null,"(§ 5.6)"]
[null,"Coefficient d'importance I",null,null,null,"Justification vis-à-vis de l’effet P-∆",null,null,"(§ 5.9)"]
[null,"Coefficient S",null,null,null,"Justification des déplacements inter-étages",null,null,"(§ 5.10)"]
[null,"Type de contreventement",null,null,null,"Hypothèse des liaisons rigides"]
[null,"Facteur de qualité Qf"]
[null,"Force  au sommet Fl (§ 6.1.2)"]
[null,"Coef. Réducteur Nu . (§ 5.10)"]
[null,"Type de structure pour Δk (§ 5.10)"]
[]
[null,null,null,"Données des efforts",null,null,null,null,null,"Données des Déplacements",null,"Avec liaisons Rigides",null,"Sans Liaisons Rigides"]
[null,"Etages","Hauteur d'étage (m)","Masses (kg)","Forces Vx (KN)","Forces VY (KN)","Centre de masse XG (m)","Centre de masse YG (m)","Poids P(G+ΨQ) (KN)","dr Ux (cm)","dr Uy (cm)","Max Ux (cm)","Max Uy (cm)","Max Ux (cm)","Max Uy (cm)"]